ReadMe for Landis+Gyr MAP120
Package Release 4.1.14
Date: 17.07.2008


1. Description
--------------

Landis+Gyr MAP120 is designed to read and to modify parameters of all devices of the Landis+Gyr Dialog, Landis+Gyr Qualigrid and most of Landis+Gyr Domestic meter series. 
For all other service functions Landis+Gyr MAP110 must be used.


2. Most recent changes, enhancements and bug fixes
--------------------------------------------------

Changes to release 4.1.14

- Parameterisation wizard: Occasional tool crash after reset dialog removed.
- ZxQ200: Trigger sources for alarm and operational indication corrected (firmware H03 only).


Changes to release 4.1.10

- Communication: The selection of the start protocol has been moved from the advanced settings to the main window of the communication centre.

- all devices: In the register selection of the load profile the registration period average value of the instantaneous values is shown.
               This only affects the visualisation, up to know the average value has been parameterised already.

- all devices: Before the reparameterisation of a profile in the parameterisation wizard starts, a warning is shown, that the profile will be erased.

- CU:     In devices with baud rate switching on channel 2 (master with baud rate switching) the dlms transmission rate is set to the same value as the IEC start transmission rate.
- CU-Ax:  Second channel is set correctly for CU-A5.
- CU-Px:  Enhanced handling of inactive time windows.
- CU-P3x: IPT connection name can be read and changed.
- CU-P30: Compare function corrected, no differences in inactive channel anymore.
- CU-D2:  Reparameterisation of parity bit has been corrected.

- AD-xP/xG: In the clock the deviation to GMT has been added as a parameter.
- AD-xP/xG: Compare function corrected, no differences in clock and multi utility registers anymore.

- ZxG300/400: Introduction of MID accuracy classes for the active part of combi meters.
- ZxG300/400: No display of stored values possible if only active rate registers are selected for the operating display. 
- ZxG300/400: Text of parameter group W76 changed to 'Over Current Monitor Thresholds'.
- ZxG300/400: After a reparameterisation or activation of a dedicated event log it is always cleared.

- ZxD300/400: Introduction of MID accuracy classes for the active part of combi meters.
- ZxD300/400: Introduction of class 0.2 for meters with integrated interface (ZxD402CR).
- ZxD300/400: Introduction of class 0.2 for meters with 3 wire connection and 1 A nominal current.
- ZxD300/400: Parameter of the first load profile entry as well as the scaling factors are now stored correctly.
- ZxD300/400: Reparameterisation of the IEC identification string now also possible for the electrical interface.

- ZxQ200: Support of firmware H03.


Changes to release 4.0.24

- AD-xG: Maximum number of profile entries is now in line with physical memory size (firmware T22).
- AD-xG: Multi utility registers can contain electricity values (firmware T22).
- AD-xG: Settings of transparent mode adapted (firmware T21). 

- ZxQ200: Starting load 0.02% for meters with 5 A nominal current introduced.


Changes to release 4.0.20

- Operating systems: Windows Vista is now supported, Windows NT and Windows 98 have been cancelled.

- Setup: New setup program offering better upgrade possibilities for future releases.

- Translation: All files now have fixed names but are located in their own subdirectories with the corresponding country code (i.e. 'en' or 'de').
               To do a translation, an existing directory must be copied, renamed to the correct country code and all files must be translated.

- Service trees: Only devices without parameterisation tree are supported anymore.

- dlms service tree: New classes (disconnector, multi utility registers) added and several texts modified. 

- IEC service tree: Endless loop removed when selecting the profiles folder.
- IEC service tree: Readout of ZxF100 devices now also possible under load. 

- Pall devices: The order of the profile entries can be modified in all devices.

- CU-E22: Display and parameterisation of IP address mode corrected.
- CU-P3x: Support of firmware D60.
- CU-P3x: Various corrections in the handling of the IP address mode.
- CU-ADP: For all types without a second channel the adapter settings have been removed.

- AD-xG: Support of firmware T22.
- AD-xG/xP: In the parameterisation wizard the disconnector log can be reset after parameterisation.

- ZxD100AR: Display lists are now shown correctly in case of stored values without numbering.

- ZxG300/400: When switching from F- to M-connection all L2 related items are shown again.
- ZxG300/400: Edit field for the power factor threshold monitor corrected.
- ZxG300/400: In the parameterisation wizard the alert message can be reset after parameterisation.


- ZxD300/400: Support of firmware B24
- ZxD300/400: Edit field for the power factor threshold monitor corrected.
- ZxD300/400: In the parameterisation wizard the alert message can be reset after parameterisation.

- ZxQ200: The event log size can be parameterised.
- ZxQ200: Energy rate registers can be controlled also via asynchronous signals of the control matrix.


Changes to release 3.3.28

- Parameterisation wizard: Window is immediately closed if no action has been selected after parameterisation (no communication with device anymore).

- CU: Compare function is now supported.
- CU: Printout of the configuration enhanced with missing information (i.e. firmware release).
- CU: A day change in the time window settings is now accepted without leaving the field.
- CU-G3x: Error in the display of the configuration corrected.
- CU-P3x: IP address of the central system can now be parameterised.

- AD-xP/xG: Support of the most recent firmware releases T01 and T21.
- AD-xP/xG: In the PING command quotation marks are now accepted.
- AD-xP/xG: Display and selection of trigger sources corrected.

- ZxG300/400: Class 0.5 for wide voltage devices and firmware P03 now supported.
- ZxG300/400: RS485 interface for wide voltage devices now supported.
- ZxG300/400: Start of load profile fixed for all devices with firmware P03 and before.
- ZxG300/400: Configuration of security attributes for security level A corrected.
- ZxG300/400: Clock status now shown correctly in the parameterisation wizard.

- ZxD300/400: Handling of error mask corrected for devices with firmware release B23.

- ZxQ200: If the IEC870 protocol is selected, the baud rate is fixed to 4800 bps (C.2 only).
- ZxQ200: Changes in the output list due to configuration changes now handled correctly (C.2 only).


Changes to release 3.3.16

- Communication: Enhancement of MAP error behaviour in case of Ethernet communication.

- Parameterisation wizard: Size of dialogue boxes modified to better support displays with a lower resolution (e.g. 800x600 pixels).

- CU: New, more user friendly display of the CU configuration.
- CU-P3x: Support of firmware D60 for pre series production.

- AD-xP/xG: Support of firmware T01 and T21 for pilot series production.

- ZxG300/400: Nominal voltage added to display lists.
- ZxG300/400: Event 9 (Daylight saving time enabled or disabled) is now triggered in both cases (after reparameterisation).
- ZxG300/400: Correction in the configuration of the electrical interfaces if RS485 and CS are fitted.
- ZxG300/400: Support of firmware P04 and ZFG300/400 for pilot series production.

- ZxD300/400: Maximal number of entries for the event log corrected if the event status register is captured.
- ZxD300/400: Event 9 (Daylight saving time enabled or disabled) is now triggered in both cases (after reparameterisation).
- ZxD300/400: Support of firmware B24 for pre series production.
- ZxD300/400: Correction of the configuration to ensure correct setting of 's' or 'S' (symmetrical connection) if the firmware release is updated from B22 to B23.

- ZxQ200: Event 9 (Daylight saving time enabled or disabled) is now triggered in both cases (after reparameterisation).


Changes to release 3.2.20

- Setup: Default directory is now 'MAP120_<release>' to avoid unintentional overwriting of former releases.

- Communication: The serial interface can be operated with 8 or 9 data bits (enhanced communication settings).

- CU with RS232: In case of an external modem the communication speed between the CU and the modem is now being read.
- CU-P2x: Reparameterisation between dynamic and fixed IP address again possible.

- AD-xP/xG: Support of firmware T01 and T21 for pre series production of Advantis 2.0.
- AD-xP/xG: Compressed output data format for profiles now selectable.

- ZxD300/300: Change in security system settings for better parameterisation of billing period reset table.

- ZxQ200: New configuration of demand measurement: Reactive demand now possible as well as apparent demand.

- ZMG300/400: Selection and parameterisation of reverse stop in measurement channels corrected.
- ZMG300/400: Adaptation of nominal voltage for meters with wide voltage range now possible.

- ZxH400: Selection and parameterisation of reverse stop in measurement channels corrected.
- ZxH400: Control matrix is now displayed completely.


Changes to release 3.2.12

- Parameterisation Trees: Number of pages corrected in printout.


Changes to release 3.2.10

- Communication: In all connection types the network delays can be activated.

- Parameterisation wizard: Clock changes are now executed in the same step as the ID number changes.
- Parameterisation wizard: Actions after reparameterisation have been accelerated.

- ID codes: If the rate number is changed all linked ID codes are now updated accordingly.
- Printout: Various enhancements in the printout.

- CU with RS232: In case of an external modem the communication speed between the CU and the modem can be defined.
- CU-P2x: A user name and a password for the login in the GPRS network can be defined.

- ZxD100AR: Support of firmware I06.

- ZxD300/400: Format of time stamps for R5/R6 commands now also visible in the load profile.
- ZxD300/400: Configuration change to ensure the correct setting of 's' or 'S'.
- ZxD300/400: Load profile configuration is also checked in case of reparameterisation. 

- ZxQ200: C.2 now possible with CT/VT correction.
- ZxQ200: Text correction for the lower range of the additional power supply:'24 - 125 VAC/DC' instead of '24 - 60 VDC' 
- ZxQ200: Reactive demand registers removed in case of apparent power.
- ZxQ200: Calculation of instantaneous THD adapted.

- ZMG300/400: New type with wide voltage range (120/208 .. 240/415 V) available. 
- ZMG300/400: Instantaneous power can now be selected in the load profile.
- ZMG300/400: New PISTA values for the different variants of fraud detection.

- ZxH400: Support of firmware Q03 with 58 V variant and three wire connection.


Changes to release 3.1.12

- ZxD300/300: Support of Chinese display.

- ZxQ: Resolution of delta registers in test mode is now set to '000.00000'.


Changes to release 3.1.10

- ZxD300/400: Maximum current 6 A added again.


Changes to release 3.1.08

- all devices: MID accuracy classes A,B,C for active energy meters introduced.

- AD-xP/xG: Support of firmware T00 and T20.

- ZxD300/400: Class 0.2 with anti tampering introduced.
- ZxD300/400: Special days of TOU are shown again in all cases.
- ZxD300/400: Trigger sources of events are stored correctly again.

- ZxQ200: Minimum primary current lowered to 20 A.


Changes to release 3.0.24

- Communication: Enhancement of MAP behaviour in case of communication breaks.
- Communication: Settings of a new communication profile are stored for the first time.

- dlms tree: Various objects added or enhanced.

- CU: Support of firmware D51.

- ZxD100AR: Support of firmware I05.

- ZxD300/400: Event 13 can now generate an entry in the event log in case of disappearance.
- ZxD300/400: Terminals for additional power supply as well as passwords P1 and W5 now visible in certification feature list.
- ZxD300/400: Enhancement of list of errors which can be cleared under the utility seal (B23 only).
- ZxD300/400: Reparameterisation of devices with reduced functionality (e.g. without SMS) enhanced.

- ZxQ200: Averaging of instantaneous values (e.g. voltage, current) corrected in the load profile.
- ZxQ200: Maximum demand now possible with reactive energy.

- ZMG300/400: Support of firmware P03

- ZMH400: Support of firmware Q02


Changes to release 3.0.20

- Communication: Support of bluetooth reading head PMR_1A of meter2cash.
- Communication: Handling of list with IP addresses corrected.
- Communication: All functions now fully available under security level E.

- CU: Change of IP address mode, GPRS username and password for E and P type devices now supported.
- CU: Parameterisation tree for firmware D41 added.
- CU: Parameterisation wizard enhanced to allow changes of modem initialisation strings.

- ZMG300/400: Support of firmware P02.

- ZxD300/400: Support of firmware B23.

- ZxQ200: Quadrant assignment of measurement channel 20 (EFR) corrected: (QI + QII) - (QIII + QIV).


Changes to release 3.0.16

- ZxQ200: Correction of primary data of meters with voltage direct connection.


Changes to release 3.0.14

- New parameterisation wizard with enhanced functionality for all meters and communication units:
  - Actions before and after parameterisation can be selected.
  - Selective parameterisation of the TOU within a device series.
  - Reparameterisation of the security system.

  This wizard replaces the existing parameterisation trees and part of the service trees.
  In future all service functions only will be available in Landis+Gyr MAP110.

- GSM installation tree removed, will be available only in Landis+Gyr MAP110.

- Communication: IEC communication via channel 2 of the CU-E2x is now working.
- Communication: Access level 'E' now available in professional edition.
- Communication: Enhanced behaviour of MAP-Tool after communication abort by the user.

- Service tree: Multiple parameterisations of passwords possible again.

- Parameterisation and service tree: Parameterisation of devices without serial number now possible.

- dlms tree: Various corrections and enhancements for the display of the status words in the profiles and for the text display of the OBIS codes. 
- dlms tree: Attribute 'phonelist' of the object 'auto dial' corrected and simple visualisation of the TOU (ID numbers) added.
- dlms tree CU: Service 'Activate new parameters' is working now.
- dlms tree CU: Object 'auto answer' now visible in CU-Ax with external modem support as well as in CU-Exx.

- CU-Exx: Number of rings in time window adapted.

- ZxD300/400: Size of load profile memory reduced by 1 page (B21 und B22).
- ZxD300/400: Frequency can't be parameterised anymore for series 2 devices since this is not supported by the devices.
- ZxD300/400: Printout of the number of entries of the profiles added.
- ZxD300/400: Parameterisation of devices without profiles or with deactivated profiles corrected.
- ZxD300/400: Enhancement of input of billing period table.
- ZxD300/400: Protocol and baud rate for interface board 'c7' now selectable.

- ZxQ200: New calculation method for apparent energy (ignore leading reactive)
- ZxQ200: Energy delta values over billing period now available.
- ZxQ200: Stored values can be shown in operating display.
- ZxQ200: Stored values profile available for c.4 and c.6.
- ZxQ200: Changes in calculation of loss resistors and pulse constants in case of three wire connection.
- ZxQ200: Iron resistors now have a resolution of 2 decimal places.
- ZxQ200: Parameterisation of meter constant U2 for voltages between 120 and 190 V added.
- ZxQ200: Additional display of meter constants for losses based on effective resistors.
- ZxQ200: THD OBIS codes now can be used for display.
- ZxQ200: Maximum frequency of pulse outputs enhanced to 24 Hz.
- ZxQ200: Parameterisation of devices without profiles or with deactivated profiles corrected.
- ZxQ200: Calculation and display of iron losses enhanced.
- ZxQ200: New type with voltage direct connection introduced.

- All known errors of beta releases 3.0.xx have been corrected.

Changes to release 2.5.18

- ZxD100AR: Support of firmware I04.
- ZxD100AR: Configuration with 1 input and 1 output: Correction of signal assignment of the static output.

- ZxD300/400: Reparameterisation of devices without SMS enhanced.


Changes to release 2.5.14

- Communication: Direct communication via Ethernet with the TCP/IP protocol implemented but not yet tested.

- dlms tree: Attribute 'mode' of class 28 'auto answer' corrected and set to read only.
- dlms tree: IP address mode of class 42 'IP setup' is now displayed correctly.

- CU: Load and save of service tree corrected.
- CU: Settings of channel 1 for all Z1 modules can be changed now.

- ZxD300/400: Support of new extension board '0450' with 4 outputs and additional power supply.
- ZxD300/400: OBIS code for gas and water of external pulse inputs corrected.
- ZxD300/400: Reparameterisation of devices without profiles enhanced.

- ZxQ200: Support of ZPQ meters.
- ZxQ200: Support of external PQ module.
- ZxQ200: Register resolution for secondary data meters adapted.
- ZxQ200: Lower limit of primary current changed to 50 A.
- ZxQ200: Delay time of current monitoring can now be parameterised and is not fixed anymore to 10 s.
- ZxQ200: Reparameterisation of devices without profiles enhanced.


Changes to release 2.5.12

- ZxD300/400: TOU again available in service tree of firmware version B14.


Changes to release 2.5.10

- Communication: Enhancement of MAP error behaviour, especially when using modems.
- Communication: Support of bluetooth reading head PMR_1 of meter2cash.

- Parameterisation tree: Printout of outputs of control table adapted to display: immediate change = '<- --' , changes synchronous to end of period = '<- \-'
- Parameterisation tree: In all profiles the OBIS logical name instead of the display code is shown for the captured objects.
- Parameterisation tree: Firmware version is checked again before parameterisation.
- Parameterisation tree: After a parameterisation only the changed values are verified => parameterisation process should run faster.

- dlms tree: The following classes for communication setup are now supported:
	   - 27: Modem configuration
	   - 28: Auto answer
	   - 29: Auto dial
	   - 41: tcp setup
	   - 42: IP setup
	   - 43: Ethernet setup
	   - 45: GPRS modem setup
- dlms tree: In the profiles the various status registers with the same OBIS code but different attribute numbers are named differently.
- dlms tree: The manufacturer specific object 'Meter Functions' is also shown in the standard view not only in enhanced Landis+Gyr view.
- dlms tree: Unit and scaler of all registers are shown more comprehensively.
- dlms tree: Pulse input values in profiles are scaled now correctly.

- ZxD100AR: Support of new software I03.
- ZxD100AR: Setting of the integration period is shown correctly after parameterisation.

- ZxD300/400: The size of the hdlc transmission buffer can be selected for all interfaces now (as in CU).
- ZxD300/400: In conjunction with scaling factors also decimal places are available. It is now possible to parameterise delta registers with the precision required.
- ZxD300/400: Indirect synchronisation of the clock via output of the control table is now working correctly. 
- ZxD300/400: Event status register again selectable for event log.
- ZxD300/400: Support of new type: ZxD402 with 60 Hz.
- ZxD300/400: Parameterisation of captured objects in profiles enhanced. The objects are written in all cases.
- ZxD300/400: Thresholds for neutral current monitoring in service tree added.
- ZxD300/400: No more error when reading energy direction contacts in service tree.
- ZxD300/400: Event trigger for neutral over current is stored and read correctly.
- ZXD300/400: Support of new extension board '0460' with 4 outputs and external DC power supply.

- ZxQ200: The size of the hdlc transmission buffer can be selected for all interfaces now (as in CU).
- ZxQ200: For measured quantities +R and -R the quadrants have been added for printout.
- ZxQ200: Transmitting contact test mode has been removed for devices with software H90.
- ZxQ200: In the list of losses also the contents of the variable registers ME23 and ME24 can be added for c.6.
- ZxQ200: Units for pulse constants adapted according to COSEM definition.
- ZxQ200: Command to reset DIP table has been added to dlms tree.
- ZxQ200: After a parameterisation of the capture period length the meter is being restarted automatically.

- CU: Type designation Q2 changed to Q22.
- CU: GSM modem type only shown for G2x and P2x types.
- CU: In all time windows the yearly repetition has been removed since this is not supported by the devices.


Changes to release 2.4.06

- Time of use: Abnormal termination of the program under Windows 98 and Windows NT in the TOU part has been eliminated.

- ZxD300/400 parameterisation tree: Instantaneous power is read back to the captured object list of the load profile.


Changes to release 2.4.04

- Parameterisation Tree: Consecutively parameterisation of several meters using the same parameterisation tree is possible again.

- Communication: Modem line is not disconnected automatically after a session break.

- dlms tree: Stored value profile and event log are visible again in the extended Landis+Gyr view for all devices.
- dlms tree: Unit of last average demand in the load profile is displayed again.

- Licensing: Start up error due to licensing problems fixed.

- ZxQ200: Firmware H02 and H90 activated for all licenses.
- ZxQ200: Inactive profiles contain at least one entry in the captured object list to ensure later reparameterisation.

- ZxD100AR: Energy registers are visible again in the extended Landis+Gyr view of the dlms tree.

- CU: In all E2x modules the alive interval in case of fixed IP addresses is activated automatically.
- CU: For all Q22 modules H02 dlms addresses have been modified.


Changes to release 2.4.02

- Licensing: The license key is invisible after input (copy protection).

- dlms tree: Monitor thresholds are read correctly now.
             Logical name for C.2.12 (timestamp of last synchronisation) added.
             Modification of various registers containing simple numbers is possible again.
             Reading of dlms load profiles without timestamp and status is possible now. The missing values are filled for display by MAP.
             Text and logical name of the last average demand are displayed correctly in the load profile.
             Additional function 'reset of energy total registers' added to the meter function object in the enhanced Landis+Gyr view.

- IEC tree: Double entries to enable and disable the energy registers in the display list have been removed.
	  After reading an empty profile any values displayed before are removed.

- Communication centre: Input of IP addresses in the phone number field possible now.
                        List entries can be removed by pressing the 'remove' button.
                        
- Parameterisation
  and  service tree: New handling of ID1, ID2, physical IEC and hdlc device address: All numbers are now stored to file and can be activated with a check box for writing.
                     Same concept for customer calibration and CT/VT correction.
                     In the header of the printout MAP120 is shown instead of MAP190.
                       
- Time of use: Data exchange via clipboard (copy and paste) between different data sets as well as between different devices is now possible.
               When adding exception days the day table number can be entered directly.
                            
- ZxD100AR: Selection of M-Bus slave type again available.

- ZxD300/400: Extension of alert trigger sources: Over current (4) and control input signal change now supported.
- ZxD300/400: Interface board 'c7' for Chinese applications now supported.
- ZxD300/400: Type designation of the RS422 interface board changed from 'c4' to 'c6'.
- ZxD300/400: Threshold of neutral current monitor is kept after editing.
- ZxD300/400: Display and selection of the integration period control via external inputs has been corrected.
- ZxD300/400: Display and selection of ID number codes has been corrected.
- ZxD300/400: Stored values of operating time registers are shown with index in display lists.
- ZxD300/400: Length of IEC identification string has been reduced to 16 characters (according to standard) instead of 20.
- ZxD300/400: Display of control matrix of former devices with firmware B12 to B14 has been corrected.
- ZxD300/400: When entering codes to the IEC-Readout list they are displayed the same way as they are given out by the device.
- ZxD300/400: Conversion of parameterisation trees from B14 to B21 possible again, enhancement for B21 to B22.
- ZxD300/400: Logical name of cumulative maximum demand registers is changed now in case of reparameterisation.

- CU: For all P2x types with firmware D50 a user name and a password for the PPP protocol can be entered.
- CU: Support of type Q22 with firmware D90.

- ZxQ200: Support of firmware H02 and H90.
- ZxQ200: Quadrant assignment for reactive energy (+R, -R) now selectable as in ZxD300/400.
- ZxQ200: Devices with 5A nominal current now support a maximal current of 200%.
- ZxQ200: Enhancement of output pulse constant range.
- ZxQ200: Parameter change of pulse output constants is recorded in event log.
- ZxQ200: Correction of LED pulses for U2 and I2, correction of pulse constant RI2.
- ZxQ200: Customer calibration always available and printed.
- ZxQ200: Range check of the CT/VT correction values.


Changes to release 2.3.08

- Time of use: The exception day table now supports a maximum of 100 entries for all devices.

- ZxD300/400: Unintended modification of display codes in the parameterisation tree is now inhibited.

- ZxD100AR: In the parameterisation tree the current MAP release is not written to the meter (no access error anymore).

- ZxQ200: Parameterisation from file for devices delivered in the past is now possible (no access error anymore).


Changes to release 2.3.04

- Licensing: The license is not hardware related anymore, i.e. you can install as many copies of the software within your organisation.
             To do so, new licenses are required. Please follow the instructions in paragraph 3.
             
- Communication centre: Communication delays now can be selected for all communication channels.
                        IEC and hdlc device addresses can be entered together (used for special multi drop applications).
	                    Various duplications have been removed.

- Device addresses: After a reparameterisation of the IEC or hdlc device address the meter is restarted automatically to activate the new addresses.

- Time of use: The position of the crosses in the printout of the day tables has been fixed.
	       After a reparameterisation of the TOU with the parameterisation tree the TOU is read back again to make sure, that the actual state of the tree is in line with the state of the device. 

- CU: Support of new CU types G2x, E2x, M2x and P2x with software D45 and D50.

- ZxD100AR: Scaling of the impulse values of the transmitting contacts is now printed correctly.

- ZxD300/400: Support of firmware version B22 in all licenses.
- ZxD300/400: Class 0.2S for series 2 devices since B22 again available.
- ZxD300/400: The delay time of the current monitor is now printed correctly.
- ZxD300/400: Variant without control inputs has been removed since it is not in the portfolio.
- ZxD300/400: Event 13 (change of the state of a control input) has been introduced to the event log for B21 and up.
- ZxD300/400: Energy register 23 and 24 are only fixed if the minimum power factor is used.
- ZxD300/400: Instantaneous active and reactive power have been introduced for B21 and up.
- ZxD300/400: Scaling of the impulse values of the transmitting contacts is now printed correctly.
- ZxD300/400: Inscription of instantaneous voltage L3 and the code for under voltage registers have been corrected in all display lists.
- ZxD300/400: Status word is not fixed in the event log anymore, only timestamp is mandatory.
- ZxD300/400: Security system: Trigger for alerts is now assigned to group W29 instead of W82.
- ZxD300/400: Codes in the display lists are printed the same way as they are shown by the device (with or without value group B).
- ZxD300/400: Proper display of integration period type after reparameterisation.
- ZxD300/400: Under-/Over voltage event L2 is now saved in parameterisation tree.
- ZxD300/400: Inscription of the phase angle reference is now done according to the actual parameterisation.

- ZxQ200: Maximum number of entries in the display lists adapted.
- ZxQ200: Synchronisation input also available for devices without rate control inputs.
- ZxQ200: Maximum frequency of the transmitting contacts has been enhanced to 6 Hz.
- ZxQ200: Customer magnitude adjustment always available.
- ZxQ200: Measurement channels 19 and 20 for energy direction are always active.

- Passwords: Handling of reparameterisation of passwords enhanced.

- Compare: Various enhancements.

- Printout: Device type in the footer is now shown correctly.


3. Upgrade
----------

3.1 Upgrade of a former Landis+Gyr MAP120 release 4.1 to the most recent release 4.1.

The newest release 4.1 automatically replaces any former release 4.1.
All data including the license and the communication profiles is kept.

Procedure: 
 1. Start the installation procedure (start setup.exe) and confirm the upgrade. 
 2. Restart the computer

3.2 Upgrade of Landis+Gyr MAP120 4.0 to the most recent release 4.1

The new release can be installed in parallel to a former release 4.0 and up.
In this case for the installation a separate directory is required.
It is strongly recommended to uninstall the old release because it will no longer be supported.
All data including the license and the communication profiles is kept.

Procedure: 
 1. Uninstall old release
 2. Install new release (start setup.exe)
 3. In case of a parallel installation select a different directory
 4. Restart the computer

3.3 Upgrade of Landis+Gyr MAP120 3.3, 3.2, 3.1, 3.0, 2.5, 2.4 or 2.3 to the most recent release 4.1

The new release can be installed in parallel to a former release 2.3 and up.
In this case for the installation a separate directory is required.
It is strongly recommended to uninstall the old release because it will no longer be supported.
All data including the license is kept.

Procedure: 
 1. Uninstall old release
 2. Install new release (start setup.exe)
 3. In case of a parallel installation select a different directory
 4. To restore the communication profiles copy the content of '\profiles' subdirectory from the old to the new release.
    Since release 4.0 the communication profiles are located in the following directories:
    Windows XP: Documents and Settings\%username%\Application Data\Landis+Gyr\MAP120\Profiles
    Windows Vista: Users\%username%\AppData\Roaming\Landis+Gyr\MAP120
 5. Restart the computer

3.4 Upgrade of Landis+Gyr MAP120 prior to 2.3

Former releases are not supported anymore, an upgrade isn't possible.


4. Supported Devices in Parameterisation Tree
---------------------------------------------

- ZxD100AR with firmware releases I06, I05, I04, I03, I02 and I01
- ZxG300/400 with firmware releases P04*, P03, P02 and P01
- ZxH400 with firmware releases Q03, Q02 and Q01
- ZxD300/400 with firmware releases B24, B23, B22, B21, B20, B14 and B13
- ZxQ200 with firmware releases H03, H02, H01 and H90
- Communication units Ax/Bx/Mx/Gx/Dx/Ex/Px with firmware releases D60, D51, D50, D45, D44, D43, D42 and D41
- Communication unit Q22 with firmware release D90
- Communication module AD-xP with firmware releases T01 and T00
- Communication module AD-xG with firmware releases T22, T21 and T20

The following devices and functions are explicitly not supported: 
- Communication units Ax/Bx/Mx and Gx with firmware release D40
- The read back and the reparameterisation of the time of use tables is not supported for firmware releases B08 and C06. MAP190 must be used for this operation.

* = device not yet released


5. Supported Devices in Service Tree
------------------------------------

- ZxD300/400 with firmware releases B08, B09, B10, B11 and B13
- ZxD100/200AT with firmware releases C06, C07, C08 and C09
- ZxD100AP with firmware releases G02 and G03


6. Known Restrictions
---------------------

- Large load profiles (> 1 day) often touch the memory boundary (RAM) of the computer. It is recommended to read large profiles day per day.
- Dlms tree: some object names are not correctly shown in the left pane (ID1.1, IEC device address). The meter is parameterised correctly and the entries are not affected neither.
- The signal names of CS15 and CS16 in control table are shown incorrectly.
- Old DDS data files must not be compatible to the new MAP120 release, so it is possible that the tool cannot load old DDS files.
- The service trees of the communication units are not supported anymore since release 3.0 (replaced by parameterisation tree and MAP110). It is not possible to convert files stored earlier, a corresponding device must be read or an export of MAP190 must be used.
- The readout of the profile size of old devices (ZxD300/400 with firmware release <B21) in the dlms tree (dlms UA view) causes an error message which can be ignored.


7. Languages
------------

Installation:                                  English and German
Tool:                                          English and German

Help about ZxD300/400 devices:                 English and German
Help about ZxQ200 devices:                     English and German
Help about ZxD100AR devices:                   English and German
Help about communication units A/B/M/G/D/E/P:  English and German
Help about ZxG300/400 devices:                 English and German
Help about AD-xG/xP communication modules:     English and German

Tool help and user manual:                     English and German


8. Operating Systems
--------------------

All tools have been tested under Windows Vista, Windows XP and Windows 2000 and should run without restrictions.


9. Licensing
-------------

The software is not protected against copying and everybody is allowed to install a demo release with limited functionality. MAP120 and MAP190 are licensed separately.
To obtain a valid license please contact your local Landis+Gyr representative.


10. Support
-----------

In case of questions on MAP tools or Landis+Gyr meters please contact your local Landis+Gyr representative.

http://www.landisgyr.com


(c) Copyright 2008 Landis+Gyr Ltd
